| **Shelf** | **Slot** | **Line Type** | **Port Range** | **Status** |
| --- | --- | --- | --- | --- |
| 1 | a | LINKAGG | 1-12 | DSA |
| 1 | a | ETHERNET | 1-12 | DSA ADN ACT OOS OOS OOS OOS OOS |
| 1 | 5 | ETHERNET | 1-12 | OOS OOS ACT ACT OOS OOS OOS OOS OOS OOS OOS OOS |
| 1 | 5 | ETHERNET | 13-24 | OOS OOS OOS OOS ACT OOS OOS OOS OOS OOS OOS OOS |
| 1 | 5 | ETHERNET | 25-36 | OOS OOS OOS OOS OOS OOS OOS OOS |
| 1 | 9 | LINKAGG | 1-12 | OOS |
| 1 | 9 | ETHERNET | 1-12 | ACT OOS OOS OOS OOS OOS OOS OOS OOS OOS OOS OOS |
| 1 | 9 | ETHERNET | 13-24 | OOS OOS OOS OOS |

Card Uptime

| **Shelf** | **Slot** | **Type** | **Card Version** | **Software Version** | **Uptime** |
| --- | --- | --- | --- | --- | --- |
| 1 | 1 | MXK-LC-GP16 | 800-03401-06-A | MXK 3.4.2.272 | 3 days, 16 hours, 4 minutes |
| 1 | 3 | MXK-LC-GP16-3 | 800-03450-04-A | MXK 3.4.2.272 | 3 days, 16 hours, 5 minutes |
| 1 | 5 | MXK-LC-AEG32 | 800-03440-01-A | MXK 3.4.2.272 | 3 days, 16 hours, 6 minutes |
| 1 | 9 | MXK-LC-AETG16 | 800-03550-01-A | MXK 3.4.2.272 | 3 days, 15 hours, 28 minutes |
| 1 | a | MXK-FC-AETG8 | 800-03383-01-A | MXK 3.4.2.272 | 3 days, 16 hours, 9 minutes |
| 1 | b | MXK-FC-AETG8 | 800-03383-02-A | MXK 3.4.2.272 | 3 days, 16 hours, 7 minutes |
| 1 | m1 | MXK-MC-TOP | 800-03576-04-B | MXK 3.4.2.272 | 3 days, 16 hours, 14 minutes |
| 1 | m2 | MXK-MC-TOP | 800-03542-02-B | MXK 3.4.2.272 | 3 days, 16 hours, 3 minutes |

| **Shelf** | **Slot** | **Type** | **Card Version** | **Software Version** | **Uptime** | **Additional Information** | **Status** |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1 | 1 | MXK-LC-GP16 | 800-03401-06-A | MXK 3.4.2.272 | 3 days, 16 hours, 4 minutes | LINE CARD W/ 16 GPON | RUNNING |
| 1 | 3 | MXK-LC-GP16-3 | 800-03450-04-A | MXK 3.4.2.272 | 3 days, 16 hours, 5 minutes | LINE CARD W/ 16 GPON and TOP | RUNNING |
| 1 | 5 | MXK-LC-AEG32 | 800-03440-01-A | MXK 3.4.2.272 | 3 days, 16 hours, 6 minutes | LINE CARD W/ 32 1G AE | RUNNING |
| 1 | 9 | MXK-LC-AETG16 | 800-03550-01-A | MXK 3.4.2.272 | 3 days, 15 hours, 28 minutes | LINE CARD W/ 16 10G AE | RUNNING |
| 1 | a | MXK-FC-AETG8 | 800-03383-01-A | MXK 3.4.2.272 | 3 days, 16 hours, 9 minutes | 14U FABRIC W/ 8x10G AE | RUNNING+TRAFFIC |
| 1 | b | MXK-FC-AETG8 | 800-03383-02-A | MXK 3.4.2.272 | 3 days, 16 hours, 7 minutes | 14U FABRIC W/ 8x10G AE | RUNNING+TRAFFIC |
| 1 | m1 | MXK-MC-TOP | 800-03576-04-B | MXK 3.4.2.272 | 3 days, 16 hours, 14 minutes | 14U MGMT W/ TOP | RUNNING |
| 1 | m2 | MXK-MC-TOP | 800-03542-02-B | MXK 3.4.2.272 | 3 days, 16 hours, 3 minutes | 14U MGMT W/ TOP | RUNNING |

SFP information

| **Interface** | **Vendor Name** | **Vendor Part Number** | **Serial Number** | **Manufacturing Date** | **Nominal Bit Rate (Gbps)** | **Upper Bit Rate Margin (%)** | **Lower Bit Rate Margin (%)** |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1-1-1-0 | FUJITSU | FIM30538 | 02688 13123 | 2008-02-10 | 0 | 0 | 0 |
| 1-1-2-0 | Ligent | LTE3680M-BH | LIGJ0348000498 | 2014-08-04 | 25 | 20 | 20 |
| 1-3-1-0 | Ligent | LTE3680M-BH | LIGJ037C003375 | 2017-12-11 | 25 | 20 | 20 |
| 1-3-4-0 | Ligent | LTE3680M-BH | LIGJ034B007438 | 2014-11-09 | 25 | 20 | 20 |

Romversion

| **card** | **ROM Version** | **Date and Time** |
| --- | --- | --- |
| 1 | MXK 3.4.2.144.007 | Aug 5 2022, 12:32:34 |
| 3 | MXK 3.4.2.144.007 | Aug 5 2022, 12:33:16 |
| 5 | MXK 3.4.2.144.007 | Aug 5 2022, 12:32:34 |
| 9 | MXK 3.1.2.212 | Jan 12 2017, 20:13:47 |
| a | MXK 3.4.2.144.007 | Aug 5 2022, 10:49:48 |
| b | MXK 3.4.2.144.007 | Aug 5 2022, 10:49:48 |
| m1 | MXK 3.4.2.144.007 | Aug 5 2022, 12:30:26 |
| m2 | MXK 3.4.2.144.007 | Aug 5 2022, 12:30:26 |

| **Component** | **Type** | **Version (ROM)** | **Version (Software)** | **Serial Number** | **Uptime** | **State** |
| --- | --- | --- | --- | --- | --- | --- |
| Line Card 1 | MXK-LC-GP16 | MXK 3.4.2.144.007 | MXK 3.4.2.272 | 8087146 | 3 days, 16 hours, 4 minutes | RUNNING |
| Line Card 3 | MXK-LC-GP16-3 | MXK 3.4.2.144.007 | MXK 3.4.2.272 | 12692025 | 3 days, 16 hours, 5 minutes | RUNNING |
| Line Card 5 | MXK-LC-AEG32 | MXK 3.4.2.144.007 | MXK 3.4.2.272 | 10886040 | 3 days, 16 hours, 6 minutes | RUNNING |
| Line Card 9 | MXK-LC-AETG16 | MXK 3.1.2.212 | MXK 3.4.2.272 | 7492860 | 3 days, 15 hours, 28 minutes | RUNNING |
| Fabric Card a | MXK-FC-AETG8 | MXK 3.4.2.144.007 | MXK 3.4.2.272 | 8089640 | 3 days, 16 hours, 9 minutes | RUNNING+TRAFFIC |
| Fabric Card b | MXK-FC-AETG8 | MXK 3.4.2.144.007 | MXK 3.4.2.272 | 8182620 | 3 days, 16 hours, 7 minutes | RUNNING+TRAFFIC |
| Management m1 | MXK-MC-TOP | MXK 3.4.2.144.007 | MXK 3.4.2.272 | 15691446 | 3 days, 16 hours, 14 minutes | RUNNING |
| Management m2 | MXK-MC-TOP | MXK 3.4.2.144.007 | MXK 3.4.2.272 | 15381780 | 3 days, 16 hours, 3 minutes | RUNNING |

GPON Port Status

Fatal Data

|  |  |
| --- | --- |
|  |  |
| Show fataldata 3 | **Timestamp**: SUN JAN 04 16:04:27 1970  **SW version**: MXK 3.4.2.144.007 MXK-LC-GP16-3, LINE CARD W/ 16 GPON and TOP (20207)  - **Task name**: taskClock  - **Errno**: 0x02020006  - **Fatal code**: 1 |
| Show fataldata 5 | **Timestamp**: THU JAN 01 00:01:57 1970  **SW version**: MXK 3.4.1.157 MXK COMMON ROM (20400)  **Task name**: tLoadModules |